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Chassis Specs: 
Freightliner 114SD 6x4 66000 DD13 

Estimate Hours: 3,100

Estimated Miles: 26,266
FEATURES:
· 80 gpm/ 3000 psi FMC water pump
· 500' x 1"-3000 PSI Piranha Jet Rodder Hose
· 10' Aluminum Telescoping Boom
· Front mounted hose reel , Articulating to driver side
· Enhanced Wireless Controls
· Water Recycling System, Includes recycling nozzle
·  Remote Control Wireless: Boom, Vacuum Breaker, Throttle & Debris body (include Hi-Dump, if applicable) Does not include remote cable pendant controls for boom or hi dump.
· Omnibus Precision Power System -Electronic Controller System Includes: a color monitor, electronic footage counter, and pressure compensated hydraulics. 
MODEL #:
 
 
VRPD3612LHAEN-P/1000
 
700 #: 700-10334
UT #: UT366
Serial #: 05229358


  
 
 
 
 
 
  
 
 
T: 888-817-1757
SalesTeam@vac-con.com
969 Hall Park Road, Green Cove Springs, FL 32043
www.vac-con.com
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